skeinforge_tools.speed ($Date: 2008/21/04 $) | index /home/enrique/Desktop/backup/babbleold/script/reprap/pyRepRap/skeinforge_tools/speed.py

`Speed is a script to set the feedrate, and flowrate.
The default 'Activate Speed' checkbox is on. When it is on, the functions described below will work, when it is off, the
functions will not be called. The speed script sets the feedrate, and flowrate. To run speed, in a shell type:
> python speed.py
The 'Extrusion Diameter over Thickness is the ratio of the extrusion diameter over the layer thickness, the default is 1.25. The
extrusion fill density ratio that is printed to the console, ( it is derived quantity not a parameter ) is the area of the extrusion
diameter over the extrusion width over the layer thickness. Assuming the extrusion diameter is correct, a high value means the
filament will be packed tightly, and the object will be almost as dense as the filament. If the value is too high, there could be too
little room for the filament, and the extruder will end up plowing through the extra filament. A low value means the filaments will
be far away from each other, the object will be leaky and light. The value with the default extrusion preferences is around 0.82.
The feedrate for the shape will be set to the 'Feedrate" preference. The speed of the orbit compared to the operating extruder
speed will be set to the "Orbital Feedrate over Operating Feedrate" preference. If you want the orbit to be very short, set the
"Orbital Feedrate over Operating Feedrate" preference to a low value like 0.1.
In the "Flowrate Choice" radio button group, if "Do Not Add Flowrate" is selected then speed will not add a flowrate to the gcode
output. If "Metric" is selected, the flowrate in cubic millimeters per second will be added to the output. If "PWM Setting" is
selected, the value in the "Flowrate PWM Setting" field will be added to the output.
The 'Perimeter Feedrate over Operating Feedrate' is the ratio of the feedrate of the perimeter over the feedrate of the infill. With
the default of 1.0, the perimeter feedrate will be the same as the infill feedrate. The 'Perimeter Flowrate over Operating Flowrate'
is the ratio of the flowrate of the perimeter over the flowrate of the infill. With the default of 1.0, the perimeter flow rate will be
the same as the infill flow rate. To have higher build quality on the outside at the expense of slower build speed, a typical
setting for the 'Perimeter Feedrate over Operating Feedrate' would be 0.5. To go along with that, if you are using a speed
controlled extruder, the 'Perimeter Flowrate over Operating Flowrate' should also be 0.5. If you are using Pulse Width Modulation
to control the speed, then you'll probably need a slightly higher ratio because there is a minimum voltage 'Flowrate PWM Setting'
required for the extruder motor to turn. The flow rate PWM ratio would be determined by trial and error, with the first trial being:
Perimeter Flowrate over Operating Flowrate ~
Perimeter Feedrate over Operating Feedrate * ( Flowrate PWM Setting - Minimum Flowrate PWM Setting )
+ Minimum Flowrate PWM Setting
The following examples speed the files Screw Holder Bottom.gcode & Screw Holder Bottom.stl. The examples are run in a terminal in the
folder which contains Screw Holder Bottom.gcode, Screw Holder Bottom.stl and speed.py. The speed function will speed if "Activate
Speed" is true, which can be set in the dialog or by changing the preferences file 'speed.csv' with a text editor or a spreadsheet
program set to separate tabs. The functions writeOutput and getSpeedChainGcode check to see if the text has been speeded,
if not they call getMultiplyChainGcode in multiply.py to get multiplied gcode; once they have the multiplied text, then they
speed.
> python speed.py
This brings up the dialog, after clicking 'Speed', the following is printed:
File Screw Holder Bottom.stl is being chain speeded.
The speeded file is saved as Screw Holder Bottom_speed.gcode
>python
Python 2.5.1 (r251:54863, Sep 22 2007, 01:43:31)
[GCC 4.2.1 (SUSE Linux)] on linux2
Type "help", "copyright", "credits" or "license" for more information.
>>> import speed
>>> speed.main()
This brings up the speed dialog.
>>> speed.writeOutput()
Screw Holder Bottom.stl
File Screw Holder Bottom.stl is being chain speeded.
The speeded file is saved as Screw Holder Bottom_speed.gcode
>>> speed.getSpeedGcode("
( GCode generated by May 8, 2008 carve.py )
( Extruder Initialization )
..
many lines of gcode
..
")
>>> speed.getSpeedChainGcode("
( GCode generated by May 8, 2008 carve.py )
( Extruder Initialization )
..
many lines of gcode
..
")`

Modules
`` |  |
__init__ skeinforge_tools.analyze cStringIO skeinforge_tools.skeinforge_utilities.euclidean | skeinforge_tools.skeinforge_utilities.gcodec skeinforge_tools.skeinforge_utilities.intercircle skeinforge_tools.skeinforge_utilities.interpret skeinforge_tools.material | math skeinforge_tools.multiply skeinforge_tools.polyfile skeinforge_tools.skeinforge_utilities.preferences | sys time

Classes
`` |  | SpeedPreferences SpeedSkein
class SpeedPreferences
`` | `A class to handle the speed preferences.`
| Methods defined here: __init__(self) `Set the default preferences, execute title & preferences fileName.` execute(self) `Speed button has been clicked.`
class SpeedSkein
`` | `A class to speed a skein of extrusions.`
| Methods defined here: __init__(self) addFlowrateLine(self, flowrateString) `Add flowrate line.` addLine(self, line) `Add a line of text and a newline to the output.` getFlowrateString(self) `Get the flowrate string.` getGcodeFromFeedrateMovement(self, feedrateMinute, point) `Get a gcode movement.` getRounded(self, number) `Get number rounded to the number of carried decimal places as a string.` getSpeededLine(self, splitLine) `Get elevated gcode line with operating feedrate.` parseGcode(self, gcodeText, speedPreferences) `Parse gcode text and store the speed gcode.` parseInitialization(self) `Parse gcode initialization and store the parameters.` parseLine(self, line) `Parse a gcode line and add it to the speed skein.`

Functions
`` |  | getSpeedChainGcode(fileName, gcodeText, speedPreferences=None) `Speed a gcode linear move text. Chain speed the gcode if it is not already speeded.` getSpeedGcode(gcodeText, speedPreferences=None) `Speed a gcode linear move text.` main() `Display the speed dialog.` writeOutput(fileName='') `Speed a gcode linear move file. Chain speed the gcode if it is not already speeded. If no fileName is specified, speed the first unmodified gcode file in this folder.`

Data
`` |  | __author__ = 'Enrique Perez (perez_enrique@yahoo.com)' __date__ = '$Date: 2008/21/04 $' __license__ = 'GPL 3.0' absolute_import = _Feature((2, 5, 0, 'alpha', 1), (2, 7, 0, 'alpha', 0), 16384)

Author
`` |  | Enrique Perez (perez_enrique@yahoo.com)