(Cupcake ABS default skeinforge profile)
(homing routing)
M104 S220 T0 (Temperature to 220 celsius)
G21 (Metric FTW)
G90 (Absolute Positioning)
G92 X0 Y0 Z0 (You are now at 0,0,0)
(You have failed me for the last time, MakerBot)
G0 Z15 (Move up for test extrusion)
M108 S255 (Extruder speed = max)
M6 T0 (Wait for tool to heat up)
G04 P5000 (Wait 5 seconds)
M101 (Extruder on, forward)
G04 P5000 (Wait 5 seconds)
M103 (Extruder off)
M01 (The heater is warming up and will do a test extrusion.  Click yes after you have cleared the nozzle of the extrusion.)
G0 Z0	(Go back to zero.)
(end of start.)
