Sensor nodes don't have a bootloader.
This folder Only exists for compatibility.
main.c simply calls the topology scan algorithm 
but does not receive or send payload.

Sensor nodes cannot prapagate payload,
they cannot be programmed by infection.

Sensor nodes must be reprogrammed using an ISP programmer.