Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language (extended) | Libraries | Comparison | Board

## analogWrite(pin, value)

#### Description

Writes an analog value (PWM wave) to a pin. Can be used to light a LED at varying brightnesses or drive a motor at various speeds. After a call to analogWrite, the pin will generate a steady wave until the next call to analogWrite (or a call to digitalRead or digitalWrite on the same pin). The frequency of the PWM signal is approximately 490 Hz.

On newer Arduino boards (including the Mini and BT) with the ATmega168 chip, this function works on pins 3, 5, 6, 9, 10, and 11. Older USB and serial Arduino boards with an ATmega8 only support analogWrite() on pins 9, 10, and 11.

#### Parameters

pin: the pin to write to.

value: the duty cycle: between 0 (always off) and 255 (always on).

#### Returns

nothing

#### Notes and Known Issues

You do not need to call pinMode() to set the pin as an output before calling analogWrite().

The PWM outputs generated on pins 5 and 6 will have higher-than-expected duty cycles. This is because of interactions with the millis() and delay() functions, which share the same internal timer used to generate those PWM outputs.

#### Example

Sets the output to the LED proportional to the value read from the potentiometer.

    int ledPin = 9;      // LED connected to digital pin 9
    int analogPin = 3;   // potentiometer connected to analog pin 3
    int val = 0;         // variable to store the read value

    void setup()
    {
      pinMode(ledPin, OUTPUT);   // sets the pin as output
    }

    void loop()
    {
      val = analogRead(analogPin);   // read the input pin
      analogWrite(ledPin, val / 4);  // analogRead values go from 0 to 1023, analogWrite values from 0 to 255
    }

#### See also

- Explanation of PWM
- pinMode
- digitalWrite
- analogRead

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Edit Page | Page History | Printable View | All Recent Site Changes