Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language (extended) | Libraries | Comparison | Board

## = assignment operator (single equal sign)

Stores the value to the right of the equal sign in the variable to the left of the equal sign.

The single equal sign in the C programming language is called the assignment operator. It has a different meaning than in algebra class where it indicated an equation or equality. The assignment operator tells the microcontroller to evaluate whatever value or expression is on the right side of the equal sign, and store it in the variable to the left of the equal sign.

#### Example

     int sensVal;                 // declare an integer variable named sensVal
    senVal = analogRead(0);       // store the (digitized) input voltage at analog pin 0 in SensVal

#### Programming Tips

The variable on the left side of the assignment operator ( = sign ) needs to be able to hold the value stored in it. If it is not large enough to hold value, the value stored in the variable will be incorrect.

Don't confuse the assignment operator [ = ] (single equal sign) with the comparison operator [ == ] (double equal signs) that evaluates whether two expressions are equal.

#### See Also

- if (comparison operators)
- char
- int
- long

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Edit Page | Page History | Printable View | All Recent Site Changes