(**** Beginning of end.txt ****)
(This file is for a MakerBot Thing-O-Matic with)
(an heated build platform)
(This file has been sliced using Skeinforge 35)
(*** begin settings ****)
(**** end settings ****)
(**** begin move to cooling position ****)
G1 X0.0 F3300.0       (move to cooling position)
G1 X0.0 Y55.0 F3300.0 (move to cooling position)
(**** end move to cooling position ****)
(**** begin filament reversal ****)
M102 (Extruder on, reverse)
G04 P2000 (Wait t/1000 seconds)
M103 (Extruder off)
(**** end filament reversal ****)
(**** begin eject ****)
M6 T0 (wait for toolhead parts (nozzle, HBP, etc) to reach temperature)
M01 (Remove the object then click yes.)
(**** end eject ****)
(**** begin cool for safety ****)
M104 S0 T0 (set extruder temperature)
(**** end cool for safety ****)
(**** end of end.txt ****)
